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	Job Ref No.
	
	
	Lab Ref No.
	

	

	1. Client Details
	
	2. Waste Details

	Company name
	
	
	Producer name
	

	Address
	
	
	Waste description
	

	
	
	
	Process generating waste
	

	
	
	
	Age of waste
	

	
	
	
	EWC code
	

	
	
	
	HP Codes
	


	Customer Contact
	
	
	Hazard Statements
	

	Tel
	
	
	
	

	Email
	
	
	Container type (e.g. IBC, stockpile)
	

	Augean Contact
	
	
	
	

	Tel
	
	
	Quantity
	

	Email
	
	
	Frequency
	

	3. Waste Composition
	
	
	

	Physical form
	
	
	Separate phases
	

	Colour
	
	
	Odour
	

	pH (or range)
	
	
	Does the waste vary?
	

	
	
	
	
	

	Substance
	Class
	Y/N
	Type / Conc.
	
	Substance
	Class
	Y/N
	Type / Conc.

	Acids

	8
	
	
	
	Oxidising agents
	(*see note)
	
	

	Alkalis

	8
	
	
	
	Reducing agents
	#
	
	

	Oils, fats, greases

	LH
	
	
	
	Nitrates / nitrites / NOx
	(*see note)
	
	

	Metals/ metal compounds

	6
	
	
	
	Fluoride
	6
	
	

	Flammable liquids (flash point <60°C)
	3
	
	
	
	Pesticides / herbicides
	6
	
	

	Flammable solids

	4.1
	
	
	
	Carcinogenic Compounds
	LH
	
	

	Halogenated solvents

	6
	
	
	
	Controlled drugs/ medicines/ APIs
	6
	
	

	Phenols/ halogenated phenols
	6
	
	
	
	Animal By-Products/ Biohazardous materials 
	(*see note)
	
	

	Styrene (please state if reacted/ inhibited)
	3
	
	
	
	Asbestos or other harmful fibrous materials 
	(*see note)
	
	

	Benzene

	3
	
	
	
	Spontaneously combustible
	(*see note)
	
	

	Isocyanates (please state if reacted/ inhibited)
	6
	
	
	
	Water/ Air reactive
	(*see note)
	
	

	Cyanides (free/ complex)

	6
	
	
	
	Explosive
	(*see note)
	
	

	Ammonia / amines / amides
	8
	
	
	
	Radioactive
	(*see note)
	
	

	Sulphur compounds

	#
	
	
	
	Flocculating or Coagulating Agents
	LH
	
	

	Detergents/ Emulsifiers

	LH
	
	
	
	PCBs/PCTs /POPS/ PFAS/PFOS/PFOA/List I/II

	6
	
	



*Note - Detail below regarding components but contact technical before sampling
	Additional
Information
	


4. Sampling Details
	Date of sample

	
	
	Sample ref/ location
	

	Sample Method (e.g. core, top, bottom)
	
	
	No. samples/degree on consolidation
	



Sections 5 and 6 to be completed by Augean’s technical, operational, or commercial teams only

5. Site Details
	Site sending sample
	
	
	Proposed disposal site
	

	Proposed disposal route/process
	
	
	
	



6. Specific Analysis Requests
	Characterisation
	
	
	Full WAC
	

	Stabilisation
	
	
	Process Modelling
	

	Visual Description
	
	
	Odour
	

	COD (mg/l)
	
	
	pH
	

	Moisture content
	
	
	Flash Point
	

	Acidity
	
	
	Alkalinity
	

	Cyanide
	Total
	
	Free
	
	
	Calorific Value (CV)
	

	Free Ammonia (mg/l)
	
	
	Formaldehyde
	

	Phenols
	
	
	Oxidising
	

	Total Metals*
	
	
	Metals Method**
	


*Sb, As, Ba, Cd, Cr (total), Cu, Pb, Hg, Mo, Ni, Se, Zn – please request Cr VI analysis if required.
** Metals analysis method should be stated if known, for landfill analysis select ICP. Other methods are XRF or Dip.

Anions
	Acetate
	
	
	Carbonate
	

	Chloride
	
	
	Fluoride
	

	Nitrate
	
	
	Nitrite
	

	Sulphate
	
	
	Other
	



Other Landfill testing
	Electrical Conductivity
	
	
	TPH (CWG)
	

	LOI (HMRC)
	
	
	LOI (WAC)
	

	TOC
	
	
	TPH/PAH
	

	Other Analysis required
	



7. DECLARATION – This form should be completed and signed by a person authorised to act on the behalf of the waste producer.
	
I declare that I have provided the best information available, and I have given an accurate description of the waste. I have not failed to mention any critical component of the waste, which, (as a consequence of omission) could harm either the health and safety of the personnel interacting with it and/or harm the environment. The waste sample is representative of the waste and will not differ significantly from the sample provided and I accept that any variance may prohibit the acceptance of the waste at the site and/or incur additional charges.



	NAME
	
	
	POSITION
	

	SIGNATURE
	
	
	DATE
	



Sections 1, 2, 3, 4, and 7 to be completed directly or by a representative of the client/ waste. All samples must be accompanied by a completed Chain of Custody including testing requirements. An incomplete form will result in delays in analysis and testing will resume once details are received. 
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